# Firewall Service Blade: Configure Static Route

You can configure the static, using this third option of the firewall service blade setup wizard, or the Configure Static Route option in the Firewall menu

## Navigation

For the Firewall Service Blade Setup Wizard:

1. Right-click the blade, then select Firewall Service Blade Setup Wizard.

2. Click Next till the Configure Static Route option, in the left pane, is selected.

For the Firewall menu:

1. Right-click the blade, then select Configure Static Route.

The following information appears:

Interface Name

IP Address

Subnet Mask

Gateway

To create a new static route, click Create.

To delete a static route, select the static route, then click Delete.

In the Firewall Service Blade Setup Wizard:

To go to the previous wizard option click Back.

To go to the next wizard option click Next.

### Interface Name

Name of the firewall interface.

### IP Address

IP address assigned to the VLAN

### Subnet Mask

Subnet mask of the VLAN IP address.

### Gateway

IP gateway for the traffic in a particular VLAN.