# IPV6 GGSN PDP Context Status

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.
2. Select MWAM module from the Category drop-down box.
3. With a device selected in the MWAM module dialog box, click Statistics.
4. Select IPV6 GGSN PDP Context Status from the Category drop-down box.

The following information appears:

> GTP V0 PDPs (cGgsnActivatedIpv6Gtpv0Pdp)

> GTP V1 PDPs (cGgsnActivatedIpv6Gtpv1Pdp)

> Active IPV6 PDPs (cGgsnActivatedIpv6Ms)

### GTP V0 PDPs (cGgsnActivatedIpv6Gtpv0Pdp)

Current number of active GPRS Tunneling Protocol (GTP) v0 IPv6 Packet Data Protocol (PDP) contexts.

### GTP V1 PDPs (cGgsnActivatedIpv6Gtpv1Pdp)

Current number of active GTP v1 IPv6 PDP contexts.

### Active IPV6 PDPs (cGgsnActivatedIpv6Ms)

Current number of active IPv6 PDP contexts.