# GGSN APN Aggregate Routes

The GGSN APN Aggregate Routes dialog box provides APN details, which include aggregation.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN APN Aggregate Routes from the Category drop-down box.

The following information is displayed:

> Internet Address Type (cgprsAccPtAggregIpAddrType)

> IP Address (cgprsAccPtAggregIpAddr)

> Net Mask (cgprsAccPtAggregIpMask)

> Row Status (cgprsAccPtAggregRowStatus)

### Internet Address Type (cgprsAccPtAggregIpAddrType)

Type of Internet address denoted by cgprsAccPtAggregIpAddr.

### IP Address (cgprsAccPtAggregIpAddr)

IP address whose network prefix is defined by cgprsAccPtAggregIpMask.

When this object is set cgprsAccPtAggregIpMask must be specified.

### Net Mask (cgprsAccPtAggregIpMask)

Net-mask pertaining to cgprsAccPtAggregIpAddr.

### Row Status (cgprsAccPtAggregRowStatus)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo.

- To delete a row, set the object to destroy.