# Foreign Agent Asymmetric Link Support Configs

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Foreign Agent Asymmetric Link Support Configs from the Category list.

The following information appears:

> Care-of-address (faSupportedCOA)

> FA Advertise (cmiFaCoaInterfaceOnly)

> FA Transmit Only Status (cmiFaCoaTransmitOnly)

### Care-of-address (faSupportedCOA)

The care-of-address supported by this foreign agent.

### FA Advertise (cmiFaCoaInterfaceOnly)

Specifies whether the foreign agent interface associated with this care-of-address (CoA) should advertise this CoA only or not. If true, other configured care-of-addresses will not be advertised.

### FA Transmit Only Status (cmiFaCoaTransmitOnly)

Specifies whether the foreign agent interface associated with this CoA is a transmit-only (uplink) interface or not. If true, the foreign agent treats all registration requests received (on any interface) for this CoA as having arrived on the care-of interface. This object can be set to true for serial care-of-interfaces only.