# Low Priority Traffic

Use this option to monitor low priority traffic transmission statistics to physical medium-dependent layer for current interval for a particular side of a particular SRP interface.

## Procedure

To access low priority traffic information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Media Dependent Current Interval Statistics dialog box appears.

2. Select Tx Physical Layer Statistics from the Category menu to display transmission physical layer statistics information.

3. Select Low Priority Traffic from the Category menu to display low priority traffic information.

Low Priority Traffic dialog box displays:

Unicast Low Priority Packets (srpRingCurUcastLowPriPktsOut)

Unicast Low Priority Octets (srpRingCurUcastLowPriOctetsOut)

Multicast Low Priority Packets (srpRingCurMcastLowPriPktsOut)

Multicast Low Priority Octets (srpRingCurMcastLowPriOctetsOut)

### Unicast Low Priority Packets (srpRingCurUcastLowPriPktsOut)

Number of low priority unicast packets going to the physical medium-dependent layer during a 15-minute interval.

### Unicast Low Priority Octets (srpRingCurUcastLowPriOctetsOut)

Number of low priority unicast octets going to the physical medium-dependent layer during a 15-minute interval.

### Multicast Low Priority Packets (srpRingCurMcastLowPriPktsOut)

Number of low priority multicast packets going to the physical medium-dependent layer during a 15-minute interval.

### Multicast Low Priority Octets (srpRingCurMcastLowPriOctetsOut)

Number of low priority multicast octets going to the physical medium-dependent layer during a 15-minute interval.

## Related Topics

Using CiscoView Interface

Using the Main Menu

Selecting Components

Configuring Devices and Components

Monitoring Devices and Components