# IMA Group Statistics

The table displays the following information:

Running Seconds

Unavailable Seconds

Near End Failures

Far End Failures

Available Tx Cell Rate

Available Rx Cell Rate

Tx Configured Links

Rx Configured Links

Tx Active Links

Rx Active Links

### RunningSecs (imaGroupRunningSecs)

Indicates the length of time since an IMA group has been in the operational state.

### UnavailableSecs (imaGroupUnavailSecs)

Indicates the number of 1-second intervals during which the IMA group traffic state machine is down.

### Near-End Failures (imaGroupNeNumFailures)

Indicates the number of times a near-end group failure (Config-Abort, Insufficient-Links) has been reported since power-up or reboot.

### Far-End Failures (imaGroupFeNumFailures)

Indicates the number of times a far-end group failure has been reported since power-up or reboot.

### Available Tx Cell Rate (imaGroupTxAvailCellRate)

Indicates the current cell rate (truncated value in cells per second) provided by the IMA group in the transmit direction, considering all the transmit links in the active state.

### Available Rx Cell Rate (imaGroupRxAvailCellRate)

Indicates the current cell rate (truncated value in cells per second) provided by the IMA group in the receive direction considering all the receive links in the active state.

### Tx Configured Links (imaGroupNumTxCfgLnks )

Indicates the number of links configured to transmit in an IMA group.

### Rx Configured Links (imaGroupNumRxCfgLnks)

Indicates the number of links configured to receive in an IMA group.

### Tx Active Links (imaGroupNumTxActLnks)

Indicates the number of links configured to transmit and are active in an IMA group.

### Rx Active Links (imaGroupNumRxActLnks)

Indicates the number of links configured to receive and are active in an IMA group.