# Monitoring Ethernet Port Status Information

The CiscoView Monitor Port window displays the following status information for an Ethernet port.

Small Pkts

Large Pkts

Misaligned Pkts

# Small Pkts (locIfInRunts)

Shows the number of input packets that were smaller than the physical media permits.

# Large Pkts (locIfInGiants)

Shows the number of input packets that were larger than the physical media permits.

# Misaligned Pkts (locIfInFrame)

Shows the number of input packets that were misaligned.