# Voice Ports

The dialog box provides information on the voice ports on the card.

## Procedure

For a FXS voice port: In the rear view, right-click the LEDs of FXS ports available in the CMM submodule.

The following information appears:

> Index (ifIndex)

> Description (ifDescr)

> Type (ifType)

> Administrative Status (ifAdminStatus)

> Operational Status (ifOperStatus)

### Index (ifIndex)

Index of the interface.

### Description (ifDescr)

Presents the interface information (for example, the product name, manufacturer, and hardware version).

### Type (ifType)

The network interface type defined in the MIB-II interface table.

For switch port ifType is ethernetcsmacd

### Administrative Status (ifAdminStatus)

The intended interface state. Possible values are up, down, and testing. You cannot set the testing value.

### Operational Status (ifOperStatus)

The current operating state of the interface.

Values are:

up (1) | The ifAdminStatus is Up.
down (2) | The ifAdminStatus is down.
testing (3) | No operational packets can be passed. You cannot set this value through SNMP.
Unknown (4) |
Dormant (5) | The interface is waiting for external actions.

###