# Transmit Side Low Priority Traffic Statistics

Use this option to monitor statistics of low priority traffic reception to physical medium-dependent layer in a particular interval for a particular side of a particular SRP interface.

## Procedure

To access low priority traffic information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Media Dependent Statistics dialog box appears.

2. Select Tx Physical Layer Statistics from the Category menu to display Transmit Physical Layer Statistics dialog box.

3. Select Low Priority Traffic from the Category menu to display low priority traffic information.

Low Priority Traffic dialog box displays:

Unicast Low Priority Packets (srpRingIntUcastLowPriPktsOut)

Unicast Low Priority Octets (srpRingIntUcastLowPriOctetsOut)

Multicast Low Priority Packets (srpRingIntMcastLowPriPktsOut)

Multicast Low Priority Octets (srpRingIntMcastLowPriOctetsOut)

### Unicast Low Priority Packets (srpRingIntUcastLowPriPktsOut)

Number of low priority unicast packets going to physical medium dependent layer in a 15-minute interval during past 24 hours.

### Unicast Low Priority Octets (srpRingIntUcastLowPriOctetsOut)

Number of low priority unicast octets going to physical medium dependent layer during a 15-minute interval during past 24 hours.

### Multicast Low Priority Packets (srpRingIntMcastLowPriPktsOut)

Number of low priority multicast packets going to physical medium dependent layer during a 15-minute interval during past 24 hours.

### Multicast Low Priority Octets (srpRingIntMcastLowPriOctetsOut)

Number of low priority multicast octets going to physical medium dependent layer during a 15-minute interval during past 24 hours.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components