# CDMA PDSN PCF and Service Option-based RP Session Update

1. Right-click the device, and select Configure.

2. Select CDMA PDSN PCF and Service Option based RP Session Update from the category list.

The following information appears:

> Pcf IP Address (cCdmaPcfSoRpSessUpdIpAddr)

> Packet Data Service Option (cCdmaPcfSoRpSessUpdServiceOption)

### Pcf IP Address (cCdmaPcfSoRpSessUpdIpAddr)

The IP address of the PCF (Packet Control Function) that serves the mobile node.

### Packet Data Service Option (cCdmaPcfSoRpSessUpdServiceOption)

A packet data service option specifies a means between the mobile station and radio network to establish and maintain cdma2000 traffic channels for packet data service.