# PIM Neighbor Details

Device > Configure > Multicasting > PIM Neighbor Details

This dialog box lists the objects specific to a Protocol Independent Multicast (PIM) neighbor device.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Neighbor ifIndex (pimNeighborIfIndex)

- Neighbor UpTime (pimNeighborUpTime)

- Neighbor Expiry Time (pimNeighborExpiryTime)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Neighbor ifIndex (pimNeighborIfIndex)

Value of ifIndex for the interface used to reach this PIM neighbor.

Neighbor UpTime (pimNeighborUpTime)

The amount time since this PIM neighbor last became a neighbor of the local router.

Neighbor Expiry Time (pimNeighborExpiryTime)

Minimum amount of time remaining before this PIM neighbor is aged out.