# Multiple Address Assignment

## Navigation

To access the Multiple Address Assignment dialog box:

1. Right-click the device.

2. Select Configure > Interface Address Table - Multiple IP Address

The following information is displayed:

- Interface Index (ciiIPAddressIfIndex)
- Internet address Type (ciiIPAddressType)
- Internet Protocol address (ciiIPAddress)
- Prefix Length (ciiIPIfAddressPrefixLength)
- Broadcast Address (ciiIPIfAddressBroadcast)
- IP Address Category (ciiIPIfAddressCategory)

### Interface Index (ciiIPAddressIfIndex)

Index value which uniquely identifies the interface to which this entry is applicable. The value of this object is the same as the ifIndex value for the interface associated with this entry.

### Internet address Type (ciiIPAddressType)

Indicates the Internet address type for this entry's InetAddress and InetAddressPrefixLength objects.

### Internet Protocol address (ciiIPAddress)

IP address to which this entry's addressing information pertains.

### Prefix Length (ciiIPIfAddressPrefixLength)

Length of the prefix associated with this entry's IP address.

- When this object is set to zero, all addresses match.

- The address type is specified by the value of ciiIPAddressType for this entry.

Note: Since this object is equivalent to the ciiIPAddressPrefixLength object, any changes made to one will affect the other.

### Broadcast Address (ciiIPIfAddressBroadcast)

Broadcast address associated with this entry's IP address. The address type is specified by the value of ciiIPAddressType for this entry.

Note: Since this object is equivalent to the ciiIPAddressBroadcast object, any changes made to one will affect the other.

### IP Address Category (ciiIPIfAddressCategory)

Indicates this entry's IP address category. When setting this object, it must comply with the value of ciiIPAddressCategoryCap.

Note: Since this object is equivalent to the ciiIPAddressCategory object, any changes made to one will affect the other.