# CDMA PDSN Closed RP Registration Statistics - 1

## Procedure

1. Right-click the device and then select Monitor.

2. Select CDMA PDSN Closed RP Registration Statistics from the Category list.

3. Select a row and click Monitor.

4. Select CDMA PDSN Closed RP Registration Statistics - 1 from the Category list.

The following information appears:

> Incoming Call Requests (ccpcPcfRcvdIcrqs)

> Accepted Call Requests (ccpcPcfAcptdIcrqs)

> Denied Call Requests (ccpcPcfDroppedIcrqs)

> Incoming Call Replies Sent (ccpcPcfSentIcrps)

> Incoming-Call-Connected Received (ccpcPcfRcvdIccns)

> Incoming-Call-Connected Accepted (ccpcPcfAcptdIccns)

### Incoming Call Requests (ccpcPcfRcvdIcrqs)

Total number of Incoming-Call-Requests received to establish an L2TP session since the L2TP tunnel was established with PCF.

### Accepted Call Requests (ccpcPcfAcptdIcrqs)

Total number of Incoming-Call-Requests accepted since the L2TP tunnel was established with PCF.

### Denied Call Requests (ccpcPcfDroppedIcrqs)

Total number of Incoming-Call-Requests denied since the L2TP tunnel was established with PCF.

### Incoming Call Replies Sent (ccpcPcfSentIcrps)

Total number of Incoming-Call-Replies sent since the L2TP tunnel was established with PCF.

### Incoming-Call-Connected Received (ccpcPcfRcvdIccns)

Total number of Incoming-Call-Connected messages received since the L2TP tunnel was established with PCF.

### Incoming-Call-Connected Accepted (ccpcPcfAcptdIccns)

Total number of Incoming-Call-Connected messages accepted since the L2TP tunnel was established with PCF.