# SRP Configure Source

Use this option to view packet count and number of packets rejected for a source address on a particular SRP interface.

## Procedure

To access configure source information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

> > The MAC Layer Traffic dialog box appears.

2. Select SRP Configure Source from the Category menu to display configure source information.

Configure Source dialog box displays:

> Accept Packets (srpMACCountPktsBySourceFlag)

> Accept Packets from Address (srpMACCountPktsBySourceAddress)

> Last Change (srpMACSourceDiscontTimeStamp)

> Reject Packets (srpMACRejectPktsBySourceFlag)

> Reject Packets from Address (srpMACRejectPktsBySourceAddress)

## Related Topics

Using CiscoView Interface

Using the Main Menu

Selecting Components

Configuring Devices and Components

Monitoring Devices and Components

### Accept Packets (srpMACCountPktsBySourceFlag)

Shows that packets are counted for a particular source address.

### Accept Packets from Address (srpMACCountPktsBySourceAddress)

Shows the source address for which packets are counted when corresponding instance of srpMACCountPktsBySourceFlag is true.

### Last Change (srpMACSourceDiscontTimeStamp)

sysUpTime when there is a change in corresponding instances of srpMACCountPktsBySourceFlag or srpMACCountPktsBySourceAddress.

### Reject Packets (srpMACRejectPktsBySourceFlag)

Shows packets rejected for a particular source address.

### Reject Packets from Address (srpMACRejectPktsBySourceAddress)

Shows the source address for which packets are rejected when corresponding instance of srpMACCountPktsBySourceFlag is true.