# CDMA PDSN System Statistics

Use this option to view system statistics details.

## Procedure

To access CDMA PDSN System Statistics information:

1. Right-click the device and select Monitor from the popup menu.

> > Monitor device dialog box appears.

CDMA PDSN System Statistics dialog box displays:

Currents Sessions Ratio [Current Number of Sessions(cCdmaSessionTotal) Vs Max Number of Sessions (cCdmaSessionMaxAllowed)]

Current PCF Ratio [Current Number of PCF(cCdmaPcfTotal) Vs Max Number of PCF (cCdmaPcfMaxAllowed)]

Simple IP Flows (cCdmaSimpleIpFlowTotal)

Mobile IP Flows(cCdmaMobileIpFlowTotal)

Proxy MoIP Flows(cCdmaProxyMobileIpFlowTotal)

Session Failures Count (cCdmaSessionFailTotal)

Note: The following variables are available for PSDNv2.0.

Active Sessions (cCdmaActiveSessions)

Dormant Sessions (cCdmaDormantSessions)

## Related Topics

CDMA PDSN Feature Overview

CDMA PDSN PCF Statistics

CDMA PDSN Session Statistics

Registration Statistics

RP Update Statistics Information

### Currents Sessions Ratio [Current Number of Sessions(cCdmaSessionTotal) Vs Max Number of Sessions (cCdmaSessionMaxAllowed)]

Ratio of number of sessions to maximum number of sessions.

Current Number of Sessions (cCdmaSessionTotal) is total number of sessions established with system.

Max Number of Sessions (cCdmaSessionMaxAllowed) is maximum number of sessions allowed by system.

### Current PCF Ratio [Current Number of PCF(cCdmaPcfTotal) Vs Max Number of PCF (cCdmaPcfMaxAllowed)]

Ratio of number of PCF to maximum number of PCF.

Current Number of PCF (cCdmaPcfTotal) is total number of Packet control function interacting with system.

Max Number of PCF (cCdmaPcfMaxAllowed) is maximum number of PCF allowed by system.

### Simple IP Flows (cCdmaSimpleIpFlowTotal)

Number of flows using simple IP service.

### Mobile IP Flows(cCdmaMobileIpFlowTotal)

Number of flows using Mobile IP service.

### Proxy MoIP Flows(cCdmaProxyMobileIpFlowTotal)

Number of flows using proxy Mobile IP service.

### Session Failures Count (cCdmaSessionFailTotal)

Number of A10/A11 session failures occurred since Packet Data Service Node agent restarted.

sysUpTime can be polled to determine if agent was restarted.

### Active Sessions (cCdmaActiveSessions)

Number of sessions in the active state.

### Dormant Sessions (cCdmaDormantSessions)

Number of sessions in the dormant state.