# Port Configuration

Device > Configure > Error Disable Timeout > Error Disable Port Configuration

From this dialog box, you can configure whether a port placed into the error disable state is automatically reenabled after the timeout interval.

Note: This dialog box is only available on devices running Catalyst OS version 5.4 or later.

The following information is displayed:

- Module/Port (portModuleIndex/portIndex)

- ErrDisable Timeout (portErrDisableTimeOutEnable)

- Cross Bar Fall Back (SysErrDisableTimeoutEnable)

- Gl2pt Ingress Loop (SysErrDisableTimeoutEnable)

- Gl2pt Threshold Exceed (SysErrDisableTimeoutEnable)

- Broadcast Suppression (SysErrDisableTimeoutEnable)

Do one of the following:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Module/Port (portModuleIndex/portIndex)

Indicates a port's module number and port number.

ErrDisable Timeout (portErrDisableTimeOutEnable)

Indicates whether the Error Disable Timeout feature is enabled.

Cross Bar Fall Back (SysErrDisableTimeoutEnable)

Indicates whether a port enters the error disable state when a crossbar failure occurs.

Note: This field is only displayed on Catalyst 6000 devices with a Supervisor II card running Catalyst OS version 7.2.1 or later.

Gl2pt Ingress Loop (SysErrDisableTimeoutEnable)

G Layer2 protocol tunneling incoming loop value.

Note: This field is only displayed on Catalyst 6000 devices running Catalyst OS version 7.2.1 or later.

Gl2pt Threshold Exceed (SysErrDisableTimeoutEnable)

G Layer2 protocol tunneling threshold exceed value.

Note: This field is only displayed on Catalyst 6000 devices running Catalyst OS version 7.2.1 or later.

Broadcast Suppression (SysErrDisableTimeoutEnable)

Indicates whether a port enters the error disable state when broadcast suppression occurs.

Note: This field is only displayed on Catalyst 6000 devices running Catalyst OS version 7.2.1 or later.