# CDMA PDSN Closed RP Information

## Procedure

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category list.

3. Select a row and click Configure.

4. Select CDMA PDSN Closed RP Information from the Category list.

The following information appears:

> Closed RP Enabled (ccpcEnabled)

> Total Sessions (ccpcSessionTotal)

### Closed RP Enabled (ccpcEnabled)

An indication of whether Closed RP feature is enabled.

### Total Sessions (ccpcSessionTotal)

The total number of sessions currently established with this system.