# GGSN Charging Alarms

The GGSN Charging Alarms category in the Chassis Configuration dialog box provides a history of the charging gateways and all charging-related alarms.

Note This dialog can be viewed if cGtpGSNService is set to 'ggsn'.

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN Charging Alarms from the Category list.

The following information appears:

Charging Gateway ID (cgprsCgAlarmHistIndex)

Gateway Type (cgprsCgAlarmHistType)

Address Type (cgprsCgAlarmHistAddrType)

IP Address (cgprsCgAlarmHistAddress)

Alarm Severity (cgprsCgAlarmHistSeverity)

Detailed Information (cgprsCgAlarmHistInfo)

### Charging Gateway ID (cgprsCgAlarmHistIndex)

Monotonically increasing integer that indexes charging gateways and charging-related alarms. The value of this object is wrapped back to one when it reaches the maximum value of 4294967295.

### Gateway Type (cgprsCgAlarmHistType)

Type of GPRS charging gateway or charging-related alarm.

### Address Type (cgprsCgAlarmHistAddrType)

Type of internet address given in cgprsCgAlarmHistAddress.

### IP Address (cgprsCgAlarmHistAddress)

IP address that uniquely identifies the charging gateway.

### Alarm Severity (cgprsCgAlarmHistSeverity)

Indicates the severity of the alarm.

### Detailed Information (cgprsCgAlarmHistInfo)

Provides detailed information on when a GPRS charging gateway or charging-related alarm is generated.