# Active Call Status

The Active Call Status dialog box provides the details of an active call.

## Procedure

1. In the rear view, right-click the LEDs of FXS ports available in the CMM submodule.

2. Select Active Call Status from the popup menu. The Active Call Status dialog box appears.

The following information is shown:

> Destination-Address (callActivePeerAddress)

> Connect Time (callActiveConnectTime)

> Call State (callActiveCallState)

> Call Origin (callActiveCallOrigin)

> Charged Units (callActiveChargedUnits)

> Information Type (callActiveInfoType)

### Destination-Address (callActivePeerAddress)

The number to which this call connects. If the number is not available, the value is a zero length string.

### Connect Time (callActiveConnectTime)

The time that the call is connected. If the call is not connected, this value is zero.

### Call State (callActiveCallState)

The current call state.

Values are:

unknown (1) | The call state is unknown.
connecting (2) | A connection attempt (outgoing call) is in process.
connected (3) | An incoming call is being validated.
active(4) | The call is active.

### Call Origin (callActiveCallOrigin)

The call origin.

Values are:

originate (1) |
answer (2) |
callback (3) |

### Charged Units (callActiveChargedUnits)

The number of charged units for this connection. For incoming calls or if charging information is not supplied by the switch, this value is zero.

### Information Type (callActiveInfoType)

The information type for this call.