# Transmit Side Low Priority Statistics

Dialog box displays following information:

Unicast Low Priority Packets (srpHostIntUcastLowPriPktsOut)

Unicast Low Priority Octets (srpHostIntUcastLowPriOctetsOut)

Multicast Low Priority Packets (srpHostIntMcastLowPriPktsOut)

MultiCast Low Priority Octets (srpHostIntMcastLowPriOctetsOut)

Unicast Low Priority Packets (srpHostIntUcastLowPriPktsOut)

Number of total unicast packets going to the higher layer during a 15-minute interval during the past 24 hours.

Unicast Low Priority Octets (srpHostIntUcastLowPriOctetsOut)

Number of unicast octets going to higher layer during a 15-minute interval during the past 24 hours.

Multicast Low Priority Packets (srpHostIntMcastLowPriPktsOut)

Number of multicast packets going to higher layer during a 15-minute interval during the past 24 hours.

MultiCast Low Priority Octets (srpHostIntMcastLowPriOctetsOut)

Number of multicast octets going to the higher layer during a 15-minute interval during the past 24 hours.