# SRP Interface Sides

Use this option to view SRP interface information of a prticular side.

## Procedure

Right-click the device and select Configure from the popup menu.

SRP Interface Sides dialog box displays:

Interface Side (srpMACInterfaceSide)

MAC Address of Neighbor (srpMACNeighborAddress)

Wrapped State (srpMACSideWrapped)

IPS Mode Request (srpMACIpsMgmtRequestedMode)

Current IPS Mode (srpMACIpsAutoDetectMode)

Received IPS Mode (srpMACIpsRemoteMode)

Received IPS Mode Type (srpMACIpsRemoteType)

Acive IPS Mode (srpMACIpsActiveMode)

Unwrap to Wrap Transitions (srpMACIpsWrapCounter)

Last Wrap (srpMACIpsLastWrapTimeStamp)

Last UnWrap (srpMACIpsLastUnWrapTimeStamp)

Clock Source (srpMACClockSourceMode)

Topology Timer (srpMACTopologyTimer)

### Interface Side (srpMACInterfaceSide)

Indication on the side of the interface for which this row contains information.

### MAC Address of Neighbor (srpMACNeighborAddress)

48-bit individual MAC address of the MAC neighbor.

### Wrapped State (srpMACSideWrapped)

Boolean flag that indicates node wrapped state.

### IPS Mode Request (srpMACIpsMgmtRequestedMode)

IPS mode requested by management for local node that can affect srpMACIpsActiveMode state of SRP node, according to the set of rules describing IPS protocol.

This variable value is from the following subset

{noRequest, manualSwitch, forcedSwitch}

### Current IPS Mode (srpMACIpsAutoDetectMode)

IPS mode as automatically detected by the the local node that can affect srpMACIpsActiveMode state of SRP node, according to the set of rules describing IPS protocol.

This variable value is one from the following subset

{SignalFail, SignalDegrade, WaitToRestore}

### Received IPS Mode (srpMACIpsRemoteMode)

IPS mode indicated in IPS messages. It is received by local node from other nodes on the ring. It can affect srpMACIpsActiveMode state of SRP node, according to the set of rules describing IPS protocol.

### Received IPS Mode Type (srpMACIpsRemoteType)

Indicates if srpMACIpsRemoteMode belongs to the adjacent node in case of the shortPath or belongs to the non-adjacent node in case of the longPath.

### Acive IPS Mode (srpMACIpsActiveMode)

Active IPS mode for local node, which can be changed based on combined effect of the following variables:

srpMACIpsMgmtRequestedMode

srpMACIpsAutoDetectMode

srpMACIpsRemoteMode

srpMACIpsRemoteType

according to the set of rules describing IPS protocol.

### Unwrap to Wrap Transitions (srpMACIpsWrapCounter)

Number of transitions from unwrap to wrap state.

### Last Wrap (srpMACIpsLastWrapTimeStamp)

System set up time value for the last wrap.

### Last UnWrap (srpMACIpsLastUnWrapTimeStamp)

System set up time value for the last unwrap.

### Clock Source (srpMACClockSourceMode)

Mode of SRP interface clock source.

Internal specifies the clock source mode as internal. It is used when connecting between two routers over a dark fiber or over WDM system. Internal mode is used as a default value.

Line specifies the clock source mode as line. It is used when connecting a router to Synchronous Optical NETwork (SONET) or Synchronous Digital Hierarchy (SDH) ADM.

### Topology Timer (srpMACTopologyTimer)

Topology timer on a SRP ring. Shows how frequently topology discovery messages are sent around ring to identify nodes. Toplogy discovery is always on. Default value is 10 seconds.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components