# CDMA PDSN Traffic (Octets) Statistics

This dialog displays the CDMA service level traffic statistics for octets.

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.

2. Select CDMA PDSN Traffic (Octets) Statistics from the Category list.

The following information appears:

Simple IP Kilo Octets Transmitted (cCdmaTransmittedSipKiloOctets)

Simple IP Kilo Octets Received (cCdmaReceivedSipKiloOctets)

Mobile IP Kilo Octets Transmitted (cCdmaTransmittedMipKiloOctets)

Mobile IP Kilo Octets Received (cCdmaReceivedMipKiloOctets)

Proxy Mobile IP Kilo Octets Transmitted (cCdmaTransmittedPmipKiloOctets)

Proxy Mobile IP Kilo Octets Received (cCdmaReceivedPmipKiloOctets)

SDB Marked Data Octets (cCdmaTransmittedSDBOctets)

### Simple IP Kilo Octets Transmitted (cCdmaTransmittedSipKiloOctets)

The number of simple IP data octets (in units of 1024 octets) sent to mobile stations from PDSN since system startup.

### Simple IP Kilo Octets Received (cCdmaReceivedSipKiloOctets)

The number of simple IP data octets (in units of 1024 octets) received from mobile stations since system startup.

### Mobile IP Kilo Octets Transmitted (cCdmaTransmittedMipKiloOctets)

The number of mobile IP data octets (in units of 1024 octets) sent to mobile stations from PDSN since system startup.

### Mobile IP Kilo Octets Received (cCdmaReceivedMipKiloOctets)

The number of mobile IP data octets (in units of 1024 octets) received from mobile stations since system startup.

### Proxy Mobile IP Kilo Octets Transmitted (cCdmaTransmittedPmipKiloOctets)

The number of proxy mobile IP data octets (in units of 1024 octets) sent to mobile stations since system startup.

### Proxy Mobile IP Kilo Octets Received (cCdmaReceivedPmipKiloOctets)

The number of proxy mobile IP data octets (in units of 1024 octets) received from mobile stations since system startup.

### SDB Marked Data Octets (cCdmaTransmittedSDBOctets)

The total number of SDB marked data octets sent to PCF from PDSN since system startup.