# RSVP Session Table

RSVP Session Table displays all sessions seen by a system.

The table displays the following information:

> Session Number (rsvpSessionNumber)

> Session Type (rsvpSessionType)

> Destination Address (rsvpSessionDestAddr)

> Destination Address Length (rsvpSessionDestAddrLength)

> Protocol (rsvpSessionProtocol)

> Session Port (rsvpSessionPort)

> Senders (rsvpSessionSenders)

> Receivers (rsvpSessionReceivers)

> Requests (rsvpSessionRequests)

Session Number (rsvpSessionNumber)

Number of the session. Session Number is only for SNMP Indexing. The number indicates has no relation to any protocol value.

Session Type (rsvpSessionType)

Type of the session. For example: IP4, IP6, IP6 with flow information.

Destination Address (rsvpSessionDestAddr)

Destination address used by all senders in a particular session. The value of this object may not be changed when the value of RowStatus object is active.

Destination Address Length (rsvpSessionDestAddrLength)

CIDR prefix length of the session address. The value for IP4 host is 32 and multicast addresses, and for IP6 addresses, 128.

The value of this object may not be changed when the value of the RowStatus object is active.

Protocol (rsvpSessionProtocol)

Indicates the internet protocol of the session.

The value of this object may not be changed when the value of the RowStatus object is active.

Session Port (rsvpSessionPort)

Indicates the UDP or TCP port number used as the destination port for all senders for the specific session. A protocol value of 50 (ESP) or 51 (AH) represents a virtual destination port. If the value is zero, the protocol does not have ports.

The value of this object may not be changed when the value of the RowStatus object is active.

Senders (rsvpSessionSenders)

Number of distinct senders currently known to be part of the session.

Receivers (rsvpSessionReceivers)

The number of reservations being requested of this system for the session.

Requests (rsvpSessionRequests)

Number of reservation requests this system is sending upstream for the session.