# Home Agent Registration Group - Mobile Binding Configs

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Home Agent Registration Group - Mobile Binding Configs from the Category list.

The following information appears:

> MN's Home IP Address (haMobilityBindingMN)

> MN's CoA (haMobilityBindingCOA)

> MN Identifier Type (cmiHaRegMnIdentifierType)

> MN Identifier Associated (cmiHaRegMnIdentifier)

> Bandwidth (cmiHaRegMnIfBandwidth)

> Roaming Interface Identifier (cmiHaRegMnIfID)

> Multiple Path Metric Type (cmiHaRegMnIfPathMetricType)

### MN's Home IP Address (haMobilityBindingMN)

The mobile node's home (IP) address.

### MN's CoA (haMobilityBindingCOA)

The mobile node's care-of-address. One mobile node can have multiple bindings with different care-of-addresses.

### MN Identifier Type (cmiHaRegMnIdentifierType)

The type of the mobile node's identifier.

### MN Identifier Associated (cmiHaRegMnIdentifier)

The identifier associated with the mobile node.

### Bandwidth (cmiHaRegMnIfBandwidth)

The bandwidth of the roaming interface through which the mobile node or router is registered.

### Roaming Interface Identifier (cmiHaRegMnIfID)

A unique number identifying the roaming interface through which the mobile node or router is registered. This is also used as an unique identifier for the tunnel from the home agent to the mobile router.

### Multiple Path Metric Type (cmiHaRegMnIfPathMetricType)

Specifies the metric to use when multiple path is enabled.