# CDMA PDSN Inter PCF Handoff Registration Update Failures

From this dialog box, you can view inter-Packet Control Function (PCF) handoff registration update failures.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Inter PCF Handoff Registration Update Failures.

The following information is displayed:

> Unspecified Failures (cCdmaRpUpdHandoffReaUnSpecFails)

> Administrative Failures (cCdmaRpUpdHandoffAdmProhibFails)

> MN Authentication Failures (cCdmaRpUpdHandoffMNAuthenFails)

> ID Mismatch Failures (cCdmaRpUpdHandoffIdMismatchFails)

> Bad Request Failures (cCdmaRpUpdHandoffBadReqFails)

> Note: These statistics are a result of inter-PCF handoffs.

### Unspecified Failures (cCdmaRpUpdHandoffReaUnSpecFails)

Number of updated registrations that failed because of an unspecified reason since system startup.

### Administrative Failures (cCdmaRpUpdHandoffAdmProhibFails)

Number of updated registrations that failed due to administrative prohibition since system startup.

### MN Authentication Failures (cCdmaRpUpdHandoffMNAuthenFails)

Number of updated registrations that failed due to a Mobile Node (MN) authentication failure since system startup.

### ID Mismatch Failures (cCdmaRpUpdHandoffIdMismatchFails)

Number of registrations that failed due to a registration identity mismatch since system startup.

### Bad Request Failures (cCdmaRpUpdHandoffBadReqFails)

Number of updated registrations that failed due to a poorly formed request since system startup.