# OSPF Address Range Configuration

The OSPF Address Range dialog box displays the address range details of OSPF.

## Procedure

For CiscoView versions earlier than 5.2:

1. Right-click the device. Then select Configure, or double-click the device.

2. Select Protocols from the Category list.

3. Select OSPF from the SelectProtocol list, then click the Details button. The OSPF Configuration dialog box appears.

4. Select Address Range Configuration from the Category list.

For CiscoView version 5.2 and later:

1. Right-click the device, then select Configure, or double-click the device.

2. Select Protocols from the Category list.

3. Select OSPF from the SelectProtocol list. Then click the Details button. The OSPF Configuration dialog box appears.

   Note: The left frame in the dialog box displays the categories and the right frame displays category details or a table. If a table is displayed, the variable on which the table is indexed and the key values of the index are listed below the category. Double-click the category to view the table and double-click a key value to view details of a particular row in the table.

   Multiple indexes for a table, if any, are listed below the category in a nested manner. Select a key value to view the rows of the table about that value. Select a key value of the lowest indexing variable to view the details of that particular row.

4. Select Address Range Configuration from the left pane.

The following information appears:

Range Area ID (ospfAreaRangeAreaID)

Network Address (ospfAreaRangeNet)

Subnet Mask (ospfAreaRangeMask)

Entry Validity (ospfAreaRangeStatus)

## Related Topics

OSPF Area Configuration

OSPF General Configuration

OSPF Host Configuration

OSPF Interface Configuration

OSPF Link State Database

OSPF Neighbor Configuration

OSPF Stub Area Configuration

OSPF ToS Metrics for Nonvirtual Interface

OSPF Virtual Neighbor Configuration

OSPF Virtual Interface Configuration

### Range Area ID (ospfAreaRangeAreaID)

Area within which the address range is to be found.

### Network Address (ospfAreaRangeNet)

IP address of the net or subnet as indicated by the range.

### Subnet Mask (ospfAreaRangeMask)

Subnet mask that pertains to the net or subnet.

### Entry Validity (ospfAreaRangeStatus)

Indicates the validity or invalidity of the entry. Setting it to invalid has the effect of rendering it inoperative. The internal effect (row removal) is implementation dependent.