# Environment Temperature

Device > Monitor > Environment Monitoring

From this dialog box, you can monitor the temperature of various device components.

This dialog box displays the following data:

- Description (CiscoEnvMonTemperatureStatusDescr)

- Temperature (C) (ciscoEnvMonTemperatureStatusValue)

- Status (ciscoEnvMonTemperatureState)

- Threshold Temp (C) (ciscoEnvMonTemperatureThreshold)

- Last Shutdown Temperature (C) (ciscoEnvMonTemperatureLastShutdown)

Do one of the following:

- Click OK to continue.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Description (CiscoEnvMonTemperatureStatusDescr)

Short textual description of the testpoint being monitored.

Temperature (C) (ciscoEnvMonTemperatureStatusValue)

Temperature of the testpoint.

Status (ciscoEnvMonTemperatureState)

Current state of the testpoint being monitored. There are six possible values:

- Normal: the component is running at the normal operating temperature

- Warning: the component is running slightly above the normal operating temperature

- Critical: the component is running well above the normal operating temperature

- Shutdown: the component is running at a dangerously high temperature, and the device should be shut down immediately

- Not Present: the temperature sensor is not present

- Not Functioning: the temperature sensor is not functioning properly

Threshold Temp (C) (ciscoEnvMonTemperatureThreshold)

Highest temperature the testpoint can attain before an emergency shutdown of the device is initiated.

Last Shutdown Temperature (C) (ciscoEnvMonTemperatureLastShutdown)

Temperature of the testpoint when an emergency shutdown of the device was last initiated.