# GGSN QOS

From this dialog box, you can view quality of service (QOS) statistics.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn and the value of cggsnQosMappingMethod is set to canonical.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Statistics.

4. Select GGSN QOS from the Category drop-down box.

The following information is displayed:

> Bandwidth Resource Used (cggsnQosCurrentUsedBandwidth)

> Premium Class Throughput (cggsnQosPremiumMeanThroughput)

> Normal Class Throughput (cggsnQosNormalMeanThroughput)

> Best-effort Class Throughput (cggsnQosBestEffortMeanThroughput)

### Bandwidth Resource Used (cggsnQosCurrentUsedBandwidth)

Amount of bandwidth resource used on the GGSN. This object can be retrieved only if cggsnQosMappingMethod is set to canonical(2).

### Premium Class Throughput (cggsnQosPremiumMeanThroughput)

Sum of the mean throughput of premium class QoS users on the GSN. This object can be retrieved only if cggsnQosMappingMethod is set to canonical(2).

### Normal Class Throughput (cggsnQosNormalMeanThroughput)

Sum of the mean throughput of normal class QoS users on the GSN. This object can be retrieved only if cggsnQosMappingMethod is set to canonical(2).

### Best-effort Class Throughput (cggsnQosBestEffortMeanThroughput)

Sum of the mean throughput of best-effort class QoS users on the GSN. This object can be retrieved only if cggsnQosMappingMethod is set to canonical(2).