# GGSN Service Aware Failure Statistics

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.
2. Select GGSN Service Aware Failure Statistics from the Category list.

The following information appears:

> GGSN Failures (cGgsnSATotalGgsnFailures)

> CSG Failures (cGgsnSATotalCsgFailures)

> DCCA Total Failures (cGgsnSATotalDccaFailures)

> DCCA Failures (cGgsnSARejDccaFailures)

> CSG Failures (cGgsnSARejCsgFailures)

### GGSN Failures (cGgsnSATotalGgsnFailures)

The number of GGSN failures, such as GGSN failure in communicating with the Content Service Gateway (CSG), or GGSN failure in receiving a response from the Diameter Credit Control Application (DCCA) server.

### CSG Failures (cGgsnSATotalCsgFailures)

The number of Content Service Gateway failures in communicating with the quota server.

### DCCA Total Failures (cGgsnSATotalDccaFailures)

The number of failures in the DCCA server.

### DCCA Failures (cGgsnSARejDccaFailures)

The number of Packet Data Protocol (PDP) sessions that have been rejected due to DCCA failure.

### CSG Failures (cGgsnSARejCsgFailures)

The number of rejected PDPs due to CSG failure.