# CDMA PDSN PPP Setup Stats Contd

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.
2. Select CDMA PDSN PPP Setup Stats Contd from the Category list.

The following information appears:

> LCP Negotiation Failures (cCdmaPppLcpOptionIssueFailures)

> IPCP Negotiation Failures (cCdmaPppIpcpOptionIssueFailures)

> Authentication Stage Failures (cCdmaPppAuthMaxRetransFailures)

> Successfully LCP Stage Conn (cCdmaPppLcpSuccesses)

> Successful Conn in IPCP Stage (cCdmaPppIpcpSuccesses)

> Successful Conn in Authentication Stage (cCdmaPppAuthSuccesses)

### LCP Negotiation Failures (cCdmaPppLcpOptionIssueFailures)

The total number of PPP connections terminated due to Link Control Protocol (LCP) options negotiation failure, such as call back user not negotiating the call back option.

### IPCP Negotiation Failures (cCdmaPppIpcpOptionIssueFailures)

The total number of PPP connections terminated due to Internet Protocol Control Protocol (IPCP) options negotiation failure, such as IP address negotiation.

### Authentication Stage Failures (cCdmaPppAuthMaxRetransFailures)

The total number of PPP connection requests that failed at the authentication stage after the maximum number of retransmissions since the system was last restarted.

### Successfully LCP Stage Conn (cCdmaPppLcpSuccesses)

The total number of PPP connections that entered the LCP stage successfully.

### Successful Conn in IPCP Stage (cCdmaPppIpcpSuccesses)

The total number of PPP connections that entered the IPCP stage successfully.

### Successful Conn in Authentication Stage (cCdmaPppAuthSuccesses)

The total number of PPP connections that succeeded authentication.