# Home agent mobility Table

The table displays the following information:

MN IpAddress (haMobilityBindingMN)

MN Care of Address (haMobilityBindingCOA)

Source IpAddress (haMobilityBindingSourceAddress)

Registration Flags (haMobilityBindingRegFlags)

4 LSBs of Identifier (haMobilityBindingRegIDLow )

4 MSBs of Identifier (haMobilityBindingRegIDHigh)

Total Registration Lifetime (haMobilityBindingTimeGranted)

Remaining Lifetime (haMobilityBindingTimeRemaining)

### MN IpAddress (haMobilityBindingMN)

The home IP address of the mobile node.

### MN Care of Address (haMobilityBindingCOA)

Mobile node's care-of-address. One mobile node can have multiple bindings with different care-of-addresses.

### Source IpAddress (haMobilityBindingSourceAddress)

Source IP address of the registration request as received by the home agent. This is either a mobile node's co-located care-of-address or an address of the foreign agent.

### Registration Flags (haMobilityBindingRegFlags)

Registration flags send by the mobile node.

### 4 LSBs of Identifier (haMobilityBindingRegIDLow )

Low 32 bits of identification used in the binding by the mobile node.

### 4 MSBs of Identifier (haMobilityBindingRegIDHigh)

High 32 bits of identification used in the binding by the mobile node

### Total Registration Lifetime (haMobilityBindingTimeGranted)

Lifetime, in seconds, granted to the mobile node for this registration.

### Remaining Lifetime (haMobilityBindingTimeRemaining)

Seconds remaining until the registration expires. It has the same intial value as the Total Registration Lifetime (haMobilityBindingTimeGranted), and is counted down by the home agent.