# Redundancy Status

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select category Redundancy Status.

The following information appears:

> Unit Id (cRFStatusUnitId)

> State (cRFStatusUnitState)

> Peer Unit Id (cRFStatusPeerUnitId)

> Peer Unit State (cRFStatusPeerUnitState)

> Is Primary Unit (cRFStatusPrimaryMode)

> Redundant Peer Detected (cRFStatusDuplexMode)

> Inhibit Manual Switch (cRFStatusManualSwactInhibit)

> Last Switching Reason (cRFStatusLastSwactReasonCode)

> Last Failover Time (cRFStatusFailoverTime)

> standbyHot Time (cRFStatusPeerStandByEntryTime)

### Unit Id (cRFStatusUnitId)

A unique identifier for this redundant unit. This identifier is implementation-specific but the method for selecting the id must remain consistent throughout the redundant system. Some example identifiers include: slot id, physical or logical entity id, or a unique id assigned internally by the RF subsystem.

### State (cRFStatusUnitState)

The current state of RF on this unit.

### Peer Unit Id (cRFStatusPeerUnitId)

A unique identifier for the redundant peer unit. This identifier is implementation-specific but the method for selecting the id must remain consistent throughout the redundant system. Some example identifiers include: slot id, physical or logical entity id, or a unique id assigned internally by the RF subsystem.

### Peer Unit State (cRFStatusPeerUnitState)

The current state of RF on the peer unit.

### Is Primary Unit (cRFStatusPrimaryMode)

The current state of RF on the primary unit.

### Redundant Peer Detected (cRFStatusDuplexMode)

Indicates whether the redundant peer unit has been detected. If the redundant peer unit is detected, this object is true. If the redundant peer unit has not been detected, this object is false.

### Inhibit Manual Switch (cRFStatusManualSwactInhibit)

Indicates whether a manual switch of activity is permitted. If a manual switch of activity is allowed, this object is false. If a manual switch of activity is not allowed, this object is true. Note that the value of this object is the inverse of the status of manual SWACTs. This object does not indicate whether a switch of activity is or has occurred. This object only indicates if the user-controllable capability is enabled. A switch of activity is the event in which the standby redundant unit becomes active and the previously active unit becomes standby.

### Last Switching Reason (cRFStatusLastSwactReasonCode)

The reason for the last switch of activity.

### Last Failover Time (cRFStatusFailoverTime)

The value of sysUpTime when the primary redundant unit took over as active. The value of this object will be 0 until the first switchover.

### standbyHot Time (cRFStatusPeerStandByEntryTime)

The value of sysUpTime when the peer redundant unit entered the standbyHot state. The value will be 0 on system initialization.