# GGSN Access Point PDPs

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Statistics.

4. Select GGSN Access Point Statistics from the Category drop-down box.

5. With an entry selected in the GGSN Access Point Statistics dialog box, click Monitor.

6. Select the category GGSN Access Point PDPs.

The following information is displayed:

> No of Successfully Network Initiated PDP context (cgprsAccPtSuccNetworkInitPdps)

> No of Network Initiated PDP context (cgprsAccPtNetworkInitPdps)

> PDP context deactivation procedures (cgprsAccPtGgsnDeactivatedPdps)

> PDP context deactivation procedures completed (cgprsAccPtSuccGgsDeactivatedPdps)

> Active PDP contexts Count (cgprsAccPtActivePdps)

> Upstream Payload (cgprsAccPtUpstreamTrafficVol)

> Downstream Payload (cgprsAccPtDownstreamTrafficVol)

### No of Successfully Network Initiated PDP context (cgprsAccPtSuccNetworkInitPdps)

The total number of successfully completed network initiated PDP context activation procedures.

### No of Network Initiated PDP context (cgprsAccPtNetworkInitPdps)

The total number of network initiated PDP context activation procedures.

### PDP context deactivation procedures (cgprsAccPtGgsnDeactivatedPdps)

The total number of PDP context deactivation procedures initiated by the GGSN.

### PDP context deactivation procedures completed (cgprsAccPtSuccGgsDeactivatedPdps)

The total number of successfully completed PDP context deactivation procedures initiated by the GGSN.

### Active PDP contexts Count (cgprsAccPtActivePdps)

The current number of active PDP contexts on this APN.

### Upstream Payload (cgprsAccPtUpstreamTrafficVol)

The total payload volume in upstream traffic. Data flow from MS to PDN is considered to be upstream traffic.

### Downstream Payload (cgprsAccPtDownstreamTrafficVol)

The total payload volume in downstream volume. Data flow from PDN to MS is considered as downstream traffic.