# GTP Path Statistics 5

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.
2. Select MWAM module from the Category drop-down box.
3. With a device selected in the MWAM module dialog box, click Configure.
4. Select GGSN GTP Path Table from the Category drop-down box.
5. With a table entry selected, click Monitor.
6. Select GTP Path Statistics5 from the Category drop-down box.

The following information appears:

> Deleted IPv6 PDPs (cGtpIpv6DeletedPDPs)

> IPv6 Messages Received (cGtpIpv6RcvdSigMsgs)

> IPv6 Messages Sent (cGtpIpv6SentSigMsgs)

> IPv6 PDUs Received (cGtpIpv6RcvdPDUs)

> IPv6 PDUs Sent (cGtpIpv6SentPDUs)

> IPv6 PDU Octets Received (cGtpIpv6RcvdOctets)

> IPv6 PDU Octets Sent (cGtpIpv6SentOctets)

### Deleted IPv6 PDPs (cGtpIpv6DeletedPDPs)

Total number of IPv6 Packet Data Protocol (PDP) contexts deleted on a serving GPRS support node (SGSN) path.

### IPv6 Messages Received (cGtpIpv6RcvdSigMsgs)

Total number of IPv6 signaling messages received on a SGSN path.

### IPv6 Messages Sent (cGtpIpv6SentSigMsgs)

Number of IPv6 signaling messages sent on a SGSN path.

### IPv6 PDUs Received (cGtpIpv6RcvdPDUs)

Total number of IPv6 protocol data unit (PDU) messages received on a SGSN path.

### IPv6 PDUs Sent (cGtpIpv6SentPDUs)

Total number of IPv6 PDU messages sent on a SGSN path.

### IPv6 PDU Octets Received (cGtpIpv6RcvdOctets)

Number of bytes received in an IPv6 PDU message on a SGSN path.

### IPv6 PDU Octets Sent (cGtpIpv6SentOctets)

Number of bytes sent in an IPv6 PDU message on a SGSN path.