# SSG Radius Client Table

The SSG Radius Client Table category of the Configure dialog box displays details on the service selection gateway (SSG) remote authentication dial-in user service client.

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select SSG Radius Client Table from the Category list.

The following information appears:

Radius Client Type (cssgRadiusClientAddrType)

Radius Client Address (cssgRadiusClientAddr)

Radius Client Rowstatus (cssgRadiusClientRowStatus)

### Radius Client Type (cssgRadiusClientAddrType)

Type of address stored in cssgRadiusClientAddr.

### Radius Client Address (cssgRadiusClientAddr)

Network layer address of the remote authentication dial-in user service (radius) client to which SSG acts as the radius-proxy.

### Radius Client Rowstatus (cssgRadiusClientRowStatus)

Status of the table entry.

Status can be used to create or delete conceptual rows in the table.

To create a row, set the object to createAndGo. There are no mandatory objects in a create request.

To delete a row, set the object to destroy.