# Packets

Monitoring > Packets

The following types of packet statistics can be monitored:

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- L3 Packets dropped by Policer (caqL3PacketsDropByPolicer)

- Tos value changed IP packets (caqTosChangedIpPackets)

- Cos value changed IP packets (caqCosChangedIpPackets)

- Cos value changed Non-IP packets (caqCosChangedNonIpPackets)

You can also set how often the graphs are updated.

The following list specifies buttons in this dialog box, as well as their function:

- Click Stop to end device monitoring.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

L3 Packets dropped by Policer (caqL3PacketDropByPolicer)

Layer 3 packets dropped due to policing.

Tos value changed IP packets (caqTosChangedIpPackets)

IP Packets whose ToS value has changed.

Cos value changed IP packets (caqCosChangedIpPackets)

IP Packets whose CoS value has changed.

Cos value changed Non-IP packets (caqCosChangedNonIpPackets)

Non-IP packets whose CoS value has changed.