# RSVP ADSPEC Information

The table displays following information:

> rsvpSenderAdspecBreak

> Hop Count

> Path Bandwidth

> Minimum Path Latency

> Maximum Transmission Unit

> Guaranteed Service

> rsvpSenderAdspecGuaranteedBreak

> rsvpSenderAdspecGuaranteedCtot

> rsvpSenderAdspecGuaranteedDtot

> rsvpSenderAdspecguaranteedCsum

> rsvpSenderAdspecGuaranteedDsum

> Guaranteed Hop Count

> Guaranteed Path Bandwidth

> Guaranteed Minimum Path Latency

> Guaranteed MTU

> Controlled Load Service

> rsvpSenderAdspecCtrlLoadBreak

> Controlled Load Hop Count

> Controlled Load Bandwidth

> Controlled Load Minimum Path Latency

> Controlled Load MTU

rsvpSenderAdspecBreak (rsvpSenderAdspecBreak)

Indicates the global break bit general characterization parameter from the ADSPEC. Possible values are True and False.

Value | Description
True | At least one non-IS hop was detected in the path.
False | No non-IS hops were detected.

Hop Count (rsvpSenderAdspecHopCount)

Indicates the hop count general characterization parameter from the ADSPEC. If the values is zero or nosuchvalue, an invalid bit was set or the parameter is not present.

Path Bandwidth (rsvpSenderAdspecPathBw)
(units: bits per second)

Indicates the path bandwidth estimate general characterization parameter from the ADSPEC. If the value is zero or nosuchValue, an invalid bit was set or the parameter is not present.

Minimum Path Latency (rsvpSenderAdspecMinLatency)
(units: microseconds)

Indicates the minimum path latency general characterization parameter from the ADSPEC. If the value is zero or nosuchValue, an invalid bit was set or the parameter is not present.

Maximum Transmission Unit (rsvpSenderAdspecMtu)
(units: bytes)

Indicates the composed maximum transmission unit general characterization parameter from the ADSPEC. If the value is zero or nosuchValue, an invalid bit was set or the parameter is not present.

Guaranteed Service (rsvpSenderAdspecGuaranteedSvc)

Indicates the presence of a Guaranteed Service fragment.

Value | Description
True | ADSPEC contains a guaranteed service fragment.
False | ADSPEC does not contain a guaranteed service fragment.

rsvpSenderAdspecGuaranteedBreak (rsvpSenderAdspecGuaranteedBreak)

Indicates whether a 'break' bit is set for the guaranteed service fragment. The presence of a 'break' bit indicates that one or more nodes along the path do not support the guaranteed service.

Value | Description
True | 'Break' bit is set for guaranteed service fragment.
False | 'Break' bit is not set if rsvpSenderAdspecGuaranteedSvc is True.

If false, and rsvpSenderAdspecGuaranteedSvc is True, the 'break' bit is not set. If rsvpSenderAdspecGuaranteedSvc is False, False or noSuchValue is displayed.

rsvpSenderAdspecGuaranteedCtot (rsvpSenderAdspecGuaranteedCtot)

Indicates the end-to-end composed value for the guaranteed service C parameter.

If the rsvpSenderAdspecGuaranteedSvc is True, this is the end-to-end composed value for the 'c' parameter. A value of zero or nosuchvalue indicates that an invalid bit was set or the parameter was not present.

If rsvpSenderAdspecGuaranteedSvc is false, this returns zero or noSuchValue.

rsvpSenderAdspecGuaranteedDtot (rsvpSenderAdspecGuaranteedDtot)(units:microseconds)

Indicates the end-to-end composed value for the guaranteed service D parameter. If rsvpSenderAdspecGuaranteedSvc is True, this is the end-to-end composed value for the guaranteed service D parameter. If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present.

If the rsvpSenderAdspecGuaranteedSvc is false, zero or noSuchValue is displayed.

rsvpSenderAdspecGuaranteedCsum ( rsvpSenderAdspecGuaranteedCsum )
(units:bytes)

Indicates the end-to-end composed value for the guaranteed service C parameter. If rsvpSenderAdspecGuaranteedSvc is True, this is the end-to-end composed value for the guaranteed service C parameter since the last reshaping point. If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present.

If the rsvpSenderAdspecGuaranteedSve is false, zero or noSuchValue is displayed.

rsvpSenderAdspecGuaranteedDsum ( rsvpSenderAdspecGuaranteedDsum)
(units:microseconds)

Indicates the end-to-end composed value for the guaranteed service D parameter. If rsvpSenderAdspecGuaranteedSvc is True, this is the end-to-end composed value for the guaranteed service D parameter since the last reshaping point. If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present.

If the rsvpSenderAdspecGuaranteedSve is false, zero or noSuchValue is displayed.

Guaranteed Hop count (rsvpSenderAdspecGuaranteedHopCount)

Indicates the service-specific override of the hop count general characterization parameter from the ADSPEC. If rsvpSenderAdspecGuaranteedSvc is True, this is the service-specific override of the the hop count general characterization parameter from the ADSPEC. If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present.

If the rsvpSenderAdspecGuaranteedSvc is false, zero or noSuchValue is displayed.

Guaranteed Path Bandwidth (rsvpSenderAdspecGuaranteedPathBw)
(units:bits per second)

Indicates the service-specific override of the path bandwidth estimated general characterization parameter from the ADSPEC. If rsvpSenderAdspecGuaranteedSvc is TRUE, this is the service-specific override of the path bandwidth estimate general characterization parameter from the ADSPEC. If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present.

If the rsvpSenderAdspecGuaranteedSvc is false, zero or noSuchValue is displayed.

Guaranteed Minimum Path Latency (rsvpSenderAdspecGuaranteedMinLatency)
(units:microseconds)

Indicates the service-specific override of the minimum path latency general characterization parameter from the ADSPEC. If the rsvpSenderAdspecGuaranteedSvc is true, this is the service-specific override of the minimum path latency general characterization parameter from the ADSPEC.

If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present.

If the rsvpSenderAdspecGuaranteedSvc is false, zero or noSuchValue is displayed.

Guaranteed MTU (rsvpSenderAdspecGuaranteedMtu)
(units:bytes)

Indicates the service-specific override of the composed maximum transmission unit general characterization parameter from the ADSPEC.

If rsvpSenderAdspecGuaranteedSvc is true, this is the service-specific override of the composed maximum transmission unit general characterization parameter from the ADSPEC.

If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present.

If the rsvpSenderAdspecGuaranteedSvc is false, zero or noSuchValue is displayed.

Controlled Load Service (rsvpSenderAdspecCtrlLoadSvc)

Indicates the presence of a controlled-load service fragment.

Value | Description
True | ADSPEC contains a controlled load service fragment.
False | ADSPEC does not contain a controlled load service fragment.

rsvpSenderAdspecCtrlLoadBreak (rsvpSenderAdspecCtrlLoadBreak)

Indicates whether any node along the path supports controlled-load service.

Value | Description
True | One or more nodes along the path do not support the controlled load service.
False | The break bit is not set, if rsvpSenderAdspecCtrlLoadSvc is true.

If rsvpSenderAdspecCtrlLoadSvc is false, False or noSuchValue is displayed.

Controlled Load HopCount (rsvpSenderAdspecCtrlLoadHopCount)

Indicates the services-specific override of the hop count general characterization parameter from the ADSPEC. If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present.

If the rsvpSenderAdspecCtrlLoadSvc is false, zero or noSuchValue is displayed.

Contolled Load Bandwidth (rsvpSenderAdspecCtrlLoadPathBw)
(units: bits per second)

Indicates the service-specific override of the path bandwidth estimate general characterization parameter from the ADSPEC. If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present. If the rsvpSenderAdspecCtrlLoadSvc is false, zero or noSuchValue is displayed.

Controlled Load Minimum Path Latency (rsvpSenderAdspecCtrlLoadMinLatency)
(units: microseconds)

Indicates the status of the service-specific override of the minimum path latency general characterization parameter from the ADSPEC. If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present. If the rsvpSenderAdspecCtrlLoadSvc is false, zero or noSuchValue is displayed.

Controlled Load MTU (rsvpSenderAdspecCtrlLoadMtu)
(units: bytes)

Indicates the status of the service-specific override of the composed Maximum Transmission unit general characterization parameter from the ADSPEC. If the value is zero or noSuchValue, an invalid bit was set or the parameter was not present. If rsvpSenderAdspecCtrlLoadSvc is false, zero or noSuchValue is displayed.