# Receive Side Low Priority Traffic Statistics

Dialog box displays following information:

Unicast Low Priority Packets (srpHostIntUcastLowPriPktsIn)

Unicast Low Priority Octets (srpHostIntUcastLowPriOctetsIn)

Multicast Low Priority Packets (srpHostIntMcastLowPriPktsIn)

MultiCast Low Priority Octets (srpHostIntMcastLowPriOctetsIn)

Unicast Low Priority Packets (srpHostIntUcastLowPriPktsIn)

Number of unicast packets received from higher layer during a 15-minute interval in the past 24 hours.

Unicast Low Priority Octets (srpHostIntUcastLowPriOctetsIn)

Number of unicast octets received from higher layer during a 15-minute interval in the past 24 hours.

Multicast Low Priority Packets (srpHostIntMcastLowPriPktsIn)

Number of multicast packets received from higher layer during a 15-minute interval in the past 24 hours.

MultiCast Low Priority Octets (srpHostIntMcastLowPriOctetsIn)

Number of multicast octets received from higher layer during a 15-minute interval in the past 24 hours.