# CDMA PDSN PCF and Service Option-based RP Session Update Statistics Contd

1. Right-click the device, and select Configure.
2. Select CDMA PDSN PCF and Service Option based RP Session Update from the category list.
3. Select a row and click the Monitor2 button.

The following information appears:

> Always On Registration Updates (cCdmaPcfSoRpSessUpdAlwaysOn)

> TNPDIT download Registration Updates (cCdmaPcfSoRpSessUpdRNPDIT)

> Session Parameter not Updated (cCdmaPcfSoRpSessUpdParamNotUpdated)

> Unspecified Reason Failures (cCdmaPcfSoRpSessUpdReaUnSpecFails)

> MN Authentication Failure (cCdmaPcfSoRpSessUpdMNAuthFails)

> Registration Identity Mismatch (cCdmaPcfSoRpSessUpdIdMismatFails)

> Poorly Formed Request (cCdmaPcfSoRpSessUpdBadReqFails)

### Always On Registration Updates (cCdmaPcfSoRpSessUpdAlwaysOn)

The total number of initial A11 registration updates sent due to Always On downloaded since the system was last restarted.

### TNPDIT download Registration Updates (cCdmaPcfSoRpSessUpdRNPDIT)

The total number of initial A11 registration updates sent due to TNPDIT downloaded since the system was last restarted.

### Session Parameter not Updated (cCdmaPcfSoRpSessUpdParamNotUpdated)

The number of session updates that failed due to session parameter not being updated since the system was last restarted.

### Unspecified Reason Failures (cCdmaPcfSoRpSessUpdReaUnSpecFails)

The number of session updates that failed for unspecified reason since the system was last restarted.

### MN Authentication Failure (cCdmaPcfSoRpSessUpdMNAuthFails)

The number of session updates that failed due to MN authentication failure since the system was last restarted.

### Registration Identity Mismatch (cCdmaPcfSoRpSessUpdIdMismatFails)

The number of session updates that failed due to registration identity mismatch since the system was last restarted.

### Poorly Formed Request (cCdmaPcfSoRpSessUpdBadReqFails)

The number of session updates that failed due to poorly formed request since the system was last restarted.