# Content Switching Module - Modify CSM VLAN

The Modify CSM VLAN dialog box allows you to modify the VLAN ID, VLAN type, IP address, and subnet mask of VLANs associated with the content switching module.

## Navigation

1. Right-click the blade, then select CSM Configuration....

2. Select a row, and click Modify.

The following information appears:

VLAN ID

VLAN Type

IP Address

Subnet Mask

### VLAN ID

Number assigned to a particular VLAN.

### VLAN Type

Type shows if the VLAN resides on a client or a server.

### IP Address

IP address associated with a particular VLAN.

### Subnet Mask

IP mask address associated with a particular VLAN.