# SRP Interface Sides

Use this option to view information about a particular side of spatial reuse protocol (SRP) interface.

## Procedure

1. Double-click or right-click the port and select Configure from the popup menu.

2. Select SRP Interface Sides from the Category menu to display SRP interface configuration information for a particular side.

SRP Interface Sides dialog box displays:

> Interface Side (srpMACInterfaceSide)

> MAC Address of Neighbor (srpMACNeighborAddress)

> Wrapped State (srpMACSideWrapped)

> IPS Mode Request (srpMACIpsMgmtRequestedMode)

> Currently Detected Mode (srpMACIpsAutoDetectMode)

> Received IPS Mode (srpMACIpsRemoteMode)

> Received IPS Mode Type (srpMACIpsRemoteType)

> Currently Active Mode (srpMACIpsActiveMode)

> Unwrap to Wrap Tranisitions (srpMACIpsWrapCounter)

> Last Wrap (srpMACIpsLastWrapTimeStamp)

> Last UnWrap (srpMACIpsLastUnWrapTimeStamp)

> Clock Source (srpMACClockSourceMode)

> Topology Discovery Timer (srpMACTopologyTimer)

## Related Topics

Using CiscoView Interface

Using the Main Menu

Selecting Components

Configuring Devices and Components

Monitoring Devices and Components

### Interface Side (srpMACInterfaceSide)

Interface side containing information.

### MAC Address of Neighbor (srpMACNeighborAddress)

Neighbor MAC address.

### Wrapped State (srpMACSideWrapped)

Node wrapped state.

Values are:

True (1) | Node is in wrapped state.
False (2) | Node is not in wrapped state.

### IPS Mode Request (srpMACIpsMgmtRequestedMode)

IPS mode requested by management for local node that can affect the srpMACIpsActiveMode state of the SRP node.

Values are:

noRequest |
manualSwitch |
forcedSwitch |

### Currently Detected Mode (srpMACIpsAutoDetectMode)

Current IPS mode automatically detected by local node that can affect srpMACIpsActiveMode state of the SRP node.

Values are:

signalFail |
signalDegrade |
waitToRestore |

### Received IPS Mode (srpMACIpsRemoteMode)

IPS mode in IPS messages received by local node on ring, which can affect srpMACIpsActiveMode state of SRP node.

### Received IPS Mode Type (srpMACIpsRemoteType)

Shows whether srpMACIpsRemoteMode object value belongs to adjacent or nonadjacent node.

Values are:

ShortPath (1) |
LongPath (2) |

### Currently Active Mode (srpMACIpsActiveMode)

Active IPS mode for an active node.

Value can change due to changes in:

srpMACIpsMgmtRequestedMode

srpMACIpsAutoDetectMode

srpMACIpsRemoteMode

srpMACIpsRemoteType

### Unwrap to Wrap Tranisitions (srpMACIpsWrapCounter)

Number of transitions from unwrap to wrap state.

### Last Wrap (srpMACIpsLastWrapTimeStamp)

Last wrap sysUpTime.

### Last UnWrap (srpMACIpsLastUnWrapTimeStamp)

Last unwrap sysUpTime.

### Clock Source (srpMACClockSourceMode)

SRP interface clock source mode.

Values are :

Internal | Clock source is internal. Used when connecting two routers over a dark fiber or over a WDM system.
Line | Line clock source. Used when connecting a router to SONET/SDH ADM.

### Topology Discovery Timer (srpMACTopologyTimer)

Topology timer on an SRP ring. Shows frequency of topology discovery messages sent around ring to identify nodes. Topology discovery is always on.

Default is 10 seconds. You can set value from 10 to 600 seconds.