# GGSN Access Point PDPs

## Procedure

1. Right-click the device, then select Monitor.

2. Select GGSN Access Point Statistics from the Category list.

3. Select a row and click on Monitor.

4. Select category GGSN Access Point PDPs.

The following details are displayed:

> Active PDP contexts Count (cgprsAccPtActivePdps)

> PDP context deactivation procedures completed (cgprsAccPtSuccGgsDeactivatedPdps)

> PDP context deactivation procedures (cgprsAccPtGgsnDeactivatedPdps)

> No of Network Initiated PDP context (cgprsAccPtNetworkInitPdps)

> No of Successfully Network Initiated PDP context (cgprsAccPtSuccNetworkInitPdps)

> Upstream Payload (cgprsAccPtUpstreamTrafficVol)

> Downstream Payload (cgprsAccPtDownstreamTrafficVol)

### No of Successfully Network Initiated PDP context (cgprsAccPtSuccNetworkInitPdps)

The total number of successfully completed network initiated PDP context activation procedures.

### No of Network Initiated PDP context (cgprsAccPtNetworkInitPdps)

The total number of network initiated PDP context activation procedures.

### PDP context deactivation procedures completed (cgprsAccPtSuccGgsDeactivatedPdps)

The total number of successfully completed PDP context deactivation procedures initiated by the GGSN.

### Active PDP contexts Count (cgprsAccPtActivePdps)

The current number of active PDP contexts on this APN.

### Upstream Payload (cgprsAccPtUpstreamTrafficVol)

The total payload volume in upstream traffic. Data flow from MS to PDN is considered to be upstream traffic.

### Downstream Payload (cgprsAccPtDownstreamTrafficVol)

The total payload volume in downstream volume. Data flow from PDN to MS is considered as downstream traffic.

### PDP context deactivation procedures (cgprsAccPtGgsnDeactivatedPdps)

The total number of PDP context deactivation procedures initiated by the GGSN.