# GGSN QOS Mapping

The GGSN QOS Mapping dialog box lists the active PDP contexts that have cggsnQosClass.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn and the value of cggsnQosMappingMethod is not set to none.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN QOS Mapping from the Category drop-down box.

5. With an entry selected in the GGSN QOS Mapping dialog box, click Monitor.

### PDP Contexts Count (cggsnQosCurrentPdps)

Number of PDP contexts that have this QOS class.