# User Database Table

## Navigation

1. Right-click the Service and Application Module for IP (SAMI) card and then select Configure.
2. Select SAMI module from the Category drop-down box.
3. With a device selected, click Statistics.
4. Select Content Services Gateway from the Category drop-down box.
5. Select User Database from the Category drop-down box.

The following information appears:

> VRF Name (ccsUserDbVrfName)

> IP Address Type (ccsUserDbIpAddrType)

> IP Address (ccsUserDbIpAddr)

> UDP Port (ccsUserDbPort)

> State (ccsUserDbState)

### VRF Name (ccsUserDbVrfName)

Name of the VPN routing/forwarding (VRF) instance over which communication with the user data server occurs. If no VRF instance is specified, then the global routing table is used.

### IP Address Type (ccsUserDbIpAddrType)

Indicates the address type of ccsUserDbIpAddr.

### IP Address (ccsUserDbIpAddr)

IP address of the user database.

### UDP Port (ccsUserDbPort)

UDP port configured for the user database.

### State (ccsUserDbState)

Status of the user database. There are three possible values:

> reset—The database is waiting to be recognized as being active.

> active—The database is available and processing requests.

> failed—The database has failed and is not processing requests.