# GGSN Quota Server Statistics

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Statistics button.

4. Select the category GGSN Quota Server Statistics.

The following information appears:

> Request Received From CSG (cGgsnSAQsRcvdRequests)

> Responses Received From CSG (cGgsnSAQsRcvdResponse)

> Request to CSG (cGgsnSAQsSentRequests)

> Responses to CSG (cGgsnSAQsSentResponses)

> Echo request / Node Alive From CSG (cGgsnSAQsRcvdPathRequests)

> Path Management Response (cGgsnSAQsRcvdPathResponses)

> QS Echo Request Message (cGgsnSAQsSentPathRequests)

> QS Echo Response Message (cGgsnSAQsSentPathResponses)

### Request Received From CSG (cGgsnSAQsRcvdRequests)

Indicates the number of request messages received from the Content Service Gateway (CSG). The counter is incremented when the quota server receives these messages:

- User profile request.
- Service authorization request.
- Service re-authorization request
- Content authorization request."

### Responses Received From CSG (cGgsnSAQsRcvdResponse)

Indicates the number of responses received from the Content Service Gateway for the corresponding requests.

### Request to CSG (cGgsnSAQsSentRequests)

Indicates the number of request messages sent to the Content Service Gateway. The counter is incremented for every request sent from the quota server, such as:

- Quota return request.
- Service stop request.
- User disconnect request.

### Responses to CSG (cGgsnSAQsSentResponses)

Indicates the number of echo and node alive requests received from the Content Service Gateway. Both Content Service Gateway and the quota server use echoes to detect the health of the path between them. The Content Service Gateway sends the real address while sending the request.

### Echo request / Node Alive From CSG (cGgsnSAQsRcvdPathRequests)

Indicates the number of responses received for path management request messages from the quota server.

### Path Management Response (cGgsnSAQsRcvdPathResponses)

Indicates the number of echo request messages sent by the quota server to check the health of the path between the quota server and the and Content Service Gateway.

### QS Echo Request Message (cGgsnSAQsSentPathRequests)

Indicates the number of path responses sent by the quota server. The quota server sends the node alive response to the Content Service Gateway for a node alive request and it sends the response for the echo request made by a Content Service Gateway with valid restart counter.

### QS Echo Response Message (cGgsnSAQsSentPathResponses)

Number of path responses sent by the quota server. The quota server sends a node alive response to the content server gateway for a node alive request and also sends the response with valid restart counter for an echo request made by the content server gateway.