# IPSec VPN Service Blade VLAN Setup

The IPSec VPN Service Blade VLAN Configuration category of the VPN Service Blade Access Port Mode Setup Wizard dialog box is used to configure crypto vlans.

## Procedure

1. Right-click the IPSec VPN Service Blade, then select VPN Service Blade Setup Wizard.

The following information appears:

Inside VLAN Interface

Outside Port/VLAN Interface

Click Create to configure new cryto VLAN connection.

### Inside VLAN Interface

VLAN ID of the inside interface.

### Outside Port/VLAN Interface

Name of the outside port or VLAN ID of the outside interface