# GGSN GTP Path Table

From this dialog box, you can view the path details of GGSN with SGSN or charging gateway.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN GTP Path Table from the Category drop-down box.

The following information is displayed:

> Address Type (cGtpPathAddressType)

> Address (cGtpPathAddress)

> Port (cGtpPathPort)

> GTP Version (cGtpPathVersion)

### Address Type (cGtpPathAddressType)

Type of Internet address by which cGtpPathAddress is reachable.

### Address (cGtpPathAddress)

An address that uniquely identifies a remote node to which this path is established.

### Port (cGtpPathPort)

Port on the remote node. The value zero is invalid.

### GTP Version (cGtpPathVersion)

GTP version of the path identified by cGtpPathEntry. There are two possible values:

- version0 represents GTP version 0

- version1 represents GTP version 1