# Frame Relay Circuits

The table displays the frame relay circuit information.

## Procedure

1. Right-click on the serial port and select Configure from the popup menu or double-click on the serial port. The port configuration table appears.

2. Select Frame Relay Circuits from the Category drop-down list box.

Dialog box displays following information:

> DLCI (frCircuitDlci)

> Oper State (frCircuitState)

> Circuit Creation Time (frCircuitCreationTime)

> Last Change Time (frCircuitLastTimeChange)

> Max Committed Bits (frCircuitCommittedBurst)

> Max Uncommitted Bits (frCircuitExcessBurst)

> Throughput (frCircuitThroughput)