# CDMA PDSN Cluster Controller Table

The PDSN Cluster Controller Table category of the Device Configuration dialog box allows you to view the packet data servicing node (PDSN) cluster controller details.

## Procedure

1. Right-click the device, then select Configure or double-click the device. The Device Configuration dialog box appears.

2. Select CDMA PDSN Cluster Controller Table from the Category list.

The following information appears:

Controller Address Type (cCdmaClusterCtrlAddressType)

Controller Address (cCdmaClusterCtrlAddress)

Controller Status (cCdmaClusterCtrlStatus)

### Controller Address Type (cCdmaClusterCtrlAddressType)

IP address type of a particular controller. The address type combined with the control address is used as the index to identify a unique cluster controller entry.

### Controller Address (cCdmaClusterCtrlAddress)

IP address of a particular controller. The controller address along with the address type is used as an index to identify a unique cluster controller entry.

### Controller Status (cCdmaClusterCtrlStatus)

Operational status of the cluster controller maintained by the member. Status can be:

Value | Description
1 | notConfigured
2 | configured
3 | alive