# Device Management (Catalyst 6000 series)

Configuring Device Information

Displays device configuration information.

Configuring Quality of Service Settings

Displays QoS settings for the device.

Configuration Files

Displays information about router configuration files that have been loaded from network servers.

Configuration Status

Displays configuration information for the device module.

Configuration History

Displays a table of configuration events that have affected the module.

IP Table

Lists IP address information for the switch.

IP Route

Displays IP Route Table information about possible destinations and how they can be reached.

ARP Table

Lists the corresponding IP and physical addresses for the switch.

TCP

Displays TCP configuration information for the switch.

TCP Connections

Displays information about the TCP connections on the switch.

UDP

Displays information for the UDP listeners on the device.

# Configuration Files

Device>Configure> Configuration Files

Use the Router Configuration Files feature to display information about router configuration files that have been loaded from network servers.

Network Config Boot Address (netConfigAddr)

Displays the address of the host that supplied the network configuration file for the device. The network configuration file conatins commands that apply to all network servers and terminal services on a network.

Network Config Filename (netConfigName)

Displays the name of the network configuration file that resides on the device.

Host Config Boot Address (hostConfigAdd)

Displays the IP address of the network server that supplied the host configuration file for the device. The host configuration file contains commands that are specific to the device.

Host Config Filename (hostConfigName)

Displays the name of the host configuration file used by the device.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# Configuration Status

Device>Configure>Configuration Status

The System Configuration dialog box displays system software information for the switch.

Running Last Changed (ccmHistoryRunningLastChanged)

The date and time that the running configuration was last changed. If this value is greater than the Running last Saved value, then the configuration has been changed but not saved.

Running Last Saved (ccmHistoryRunningLastSaved)

The date and time that the running configuration was last saved (written).

Startup Last Changed (ccmHistoryStartupLastChanged)

the date and time that the startup configuration was last written. In general, this is the default configuration used when the system is cold started. It could have been changed by a save of the running configuration or by a copy from elsewhere.

Maximum Event Entries (ccmHistoryMaxEventEntries)

The maximum number of entries that can be held in the History Event Table. The recommended value for implementations is 10.

Entries Bumped (ccmHistoryEvent EntriesBumped)

The number of times the oldest entry in the History Event Table was deleted to make room for a new entry.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# Configuration History

Device>Configure>Configuration History

Use the Configuration History Table to review configuration events that have affected the module.

Event Time (ccmHistoryEventTime)

The date and time the event occurred.

Command Source (ccmHistoryEventCommandSource)

The source of the command that initiated the event.

Config Source (ccmHistoryEventConfigSource)

The configuration data source for the event.

Config Destination (ccmHistoryEventConfigDestination)

The configuration data destination for the event.

Terminal Type (ccmHistoryEventTerminalType)

If the Command Source value is “commandLine,” this is the terminal type.

Terminal Number (ccmHistoryEventTerminalNumber)

If the Command Source value is “commandLine,” this is the terminal number of the looged-in user. The value is -1 if the number is not available or not applicable.

Terminal User (ccmHistoryEventTerminalUser)

If the Command Source value is “commandLine,” this is the name of the looged-in user. The value is 0 if the name is not available or not applicable.

Terminal Location (ccmHistoryEventTerminalLocation)

If the Command Source value is “commandLine,” this is the hardwired location of the terminal or the remote host for an incoming connection. The value is 0 if the location is not available or not applicable.

Command Source Address (ccmHistoryEventCommandSourceAddress)

If the Terminal Type value is “virtual,” this is the internet address of the connected system. If the Command Source value is “snmp,” this is the internet address of the requester. The value is 0.0.0.0 if the address is not available or not applicable.

Virtual Host Name (ccmHistoryEventVirtualHostName)

If the Terminal Type value is “virtual,” this is the host name of the connected system. The value is 0 if the host name is not available or not applicable.

Server Address (ccmHistoryEventServerAddress)

If the Config Source of Config Destination value is “networkTftp,” or “networkRcp,” this is the configuration file name at the storage file server. The value is 0 if the address is not applicable or not available.

Config File (ccmHistoryEventFile)

If the Config Source of Config Destination value is “networkTftp,” or “networkRcp,” this is the internet address of the storage file server. The value is 0.0.0.0 if the address is not applicable or not available.

Remote Copy (rcp) User (ccmHistoryEventRcpUser)

If the Config Source of Config Destination value is “networkRcp,” this is the remote user name. The length is 0 if the user name is not applicable or not available.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# IP Table

Device>Configure>IP Table

The IP Table dialog box displays IP address information for the switch.

Port (ipAdEntIfIndex)

Index value for the interface of this IP address.

IP Address (ipAdEntAddr)

IP address for this entity.

Subnet Mask (ipAdEntNetMask)

Subnet mask associated with this IP address.

Broadcast Format (ipAdEntBcastAddr)

Value of the least-significant bit in the IP broadcast address for this entity.

Reasm Max Size (ipAdEntReasmMaxSize)

Size, in bytes, of the largest IP datagram that this entity can reassemble from incoming fragmented datagrams.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# IP Route

Device>Configure>IP Route Table

Use the IP Route Table dialog box to review stored information about possible destinations and how to reach them. Whenever a host or gateway needs to transmit a packet, it consults the Routing Table to determine by which route it will send the datagram. Each entry in the Routing Table describes an IP route.

Destination (ipRouteDest)

Indicates the destination IP address of the route. The address 0.0.0.0 is the default.

Next Hop (ipRouteHop)

Specifies the next hop for this route.

Mask (ipRouteMask)

Displays the subnet mask for the destination address.

Routing Protocol (ipRouteProto)

Displays the protocol by which the route was learned by the system.

Port (ipRoutePort)

Displays the index of the interface through which traffic to this destination is transmitted.

Hop Count (ipRouteMetric)

Displays the number of hops (1 or 0) for this route; its meaning depends on the routing protocol.

Route Type (ipRouteType)

Displays the status or type of the route. Possible values are direct, indirect, invalid, or other. The invalid value is usually used to delete an entry. Otherwise, it indicates an error.

Route Age (ipRouteAge)

Displays the number of seconds that have elapsed since this route was last updated or validated.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# ARP Table

Device>Configure>ARP Table

The ARP Table dialog box displays the corresponding IP and physical addresses for the switch, taken from the switch's ARP table. You can edit any of these values, or delete a mapping entry from the table.

Interface (ipNetToMediaIfIndex)

Interface on which this entry's IP-address-to-physical-address mapping is effective.

Network Address (ipNetToMediaNetAddress)

IP address corresponding to the media-dependent physical address.

Physical Address (ipNetToMediaPhysAddress)

Media-dependent physical (MAC) address for this entry.

Type (ipNetToMediaType)

Type of address mapping: dynamic, static, invalid, or other.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# TCP

Device>Configure>TCP

The TCP dialog box lists TCP configuration information for the switch.

Retransmission Algorithm (tcpRtoAlgorithm)

Algorithm that determines the TCP retransmission timeout value: constant, rsre (MIL-STD-1778), vanj (Van Jacobson's algorithm), or other.

Min Retransmission Timeout (tcpRtoMin)

Minimum permitted value, in milliseconds, for the TCP retransmission timeout.

Max Retransmission Timeout (tcpRtoMax)

Maximum permitted value, in milliseconds, for the TCP retransmission timeout.

Max Connections (tcpMaxConn)

Maximum number of TCP connections this entity can support. If this number is dynamic, the value is -1.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# TCP Connections

Device>Configure>TCP Connections

The TCP Connections dialog box displays information about the TCP connections currently open on the switch. You can change the state of any connection.

Local Address (tcpConnLocalAddress)

Local IP address for this TCP connection.

Port (tcpConnLocalPort)

Local port number for this TCP connection.

Remote Address (tcpConnRemAddress)

Remote IP address for this TCP connection.

Port (tcpConnRemPort)

Remote port number for this TCP connection.

State (tcpConnState)

State of this TCP connection. Common values are listen, closed, and closing. Set this value to delete to terminate the selected connection.

Click Apply to make your changes take effect. Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# UDP

Device>Configure>UDP

The UDP dialog box displays information for the UDP listeners on the device.

Local Address (udpLocalAddress)

Local IP address for this UDP listener.

Local Port (udpLocalPort)

Local port number for this UDP listener.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.